From factory compressed oils and fats

**Discharge point value**

Q = 119 m3/day

COD = 75 mg/l

BOD5 = 50 mg/l

Total N = 20 mg/l

Total P = 4 mg/l

TSS = 50 mg/l

Oils & grease = 50 mg/l

**Industrial wastewater 2**

Q = 19m3/day

COD = 16.000mg/l

BOD5 = 8.000 mg/l

Total N = 0 mg/l

Total P = 0 mg/l

**Industrial wastewater 2**

Q = 19m3/day

COD = 300,000 mg/l

BOD5 = 300.000 mg/l

Total N = 0 mg/l

Total P = 0 mg/l

**Industrial wastewater 1**

Q = 80 m3/day

COD = 16,000 mg/l

BOD5 = 8,000 mg/l

Total N = 20 mg/l

Total P = 12 mg/l

TSS = 6000 mg/l

Oils & grease = 6000 mg/l

**Domestic wastewater**

Q = 20 m3/day

COD = 600 mg/l

BOD5 = 300 mg/l

Total N = 85 mg/l

Total P = 15 mg/l

SS = 350 mg/l