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Diagram for water 3t 20°C

‘Note: Forsizes not covered by Nomogram, please
‘contact Technical Support Department.
‘The nomogram s based on the Prandti - Coalbrook:

formula using a k factor of

HDPE_design-considerations_vo02

k=o.00mm.
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‘Approsimate values only

Factors applicable to other flow formulae are:

Hazen Williams
‘Manning

c=150





