[bookmark: _GoBack][image: ]The technique foresees three interconnected enclosures between them properly buried to maintain the thermal insulation.
1. Mix with 50% water and 50% fresh bovine manure.
2. The water in this box can be used for fertilization.
3. Or released to the subsoil, without risk to the water table.
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Passo a Passo
Técnica prevé a conexdo de trés caixas-d'agua entre si, devidamente enterradas para preservar

isolamento térmico
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llustragdo: Antonio Figueiredo

1. mistura com 50% de 4gua e 50% de esterco bovino fresco
2. A 4gua desta caixa pode ser usada para fertirrigacio...

3.... ou liberada para o subsolo, sem risco para o lencol freatico




